{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价清单","index":0,"n_rows":53,"n_cols":7,"rows_kept":53,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[7,1,7,4],[8,0,8,6],[9,0,9,6],[20,1,20,3],[20,4,20,5],[21,0,21,6],[23,6,24,6],[25,6,26,6],[27,6,28,6],[35,6,36,6],[37,6,38,6],[46,1,46,3],[46,4,46,5],[47,1,47,3],[47,4,47,5],[50,4,50,5],[51,0,51,3],[51,4,51,5],[52,0,52,6]],"flags":["formulas_cached_only"]}
["福州智慧体育公园充电项目估算清单"]
["一、设备部分"]
["1.主材清单"]
["序号","项目名称、特征","单位","数量","综合单价","合价","备注"]
[1,"800KVA箱式变电站（终端型）","台",1,null,{"v":0,"d":"0.00"},"1.含运费\n2.含税\n3.S-20油浸式全铜变压器\n4.符合GB-20052-2020、GB1094.1-2013、GB/T6451 二级能耗标准"]
[2,"YJLHV-0.6/1KV 3*150+2*70mm2","M",120,null,{"v":0,"d":"0.00"},"1.含运费\n2.含税\n3.电缆双拼\n4.符合国标GB/T 31840-2015"]
[3,"YJLHV-0.6/1KV 4*150+1*70mm2","M",230,null,{"v":0,"d":"0.00"},"1.含运费\n2.含税\n3.符合国标GB/T 31840-2015"]
[null,"主材小计：(元）",{"$nulls":3},{"v":0,"d":"0.00"},"含税"]
["二、施工部分"]
["1、高压部分"]
["序号","项目名称、特征","单位","数量","综合单价/指导价\n","合价","备注"]
[1,"箱变安装","项",1,null,{"v":0,"d":"0.00"},"含设备吊装卸货、二次搬运、开箱检查，本体就位，器身检查，垫铁及止轮器制作、安装，附件安装，接地、补漆，单体调试"]
[2,"箱变基础平台制作","项",1,null,{"v":0,"d":"0.00"},"制作箱变平台，5.3m*5m*1.2m，按布置方案要求制作"]
[3,"箱变接地系统","项",1,null,{"v":0,"d":"0.00"}]
[4,"箱变调试、试验、送电","项",1,null,{"v":0,"d":"0.00"}]
[5,"设计费","项",1,null,{"v":0,"d":"0.00"},"含施工图、竣工图等成套设计图纸"]
[6,"围栏","米",25,null,{"v":0,"d":"0.00"},"箱变围栏：1、材质：304不锈钢 2、高度不少于1.2m"]
[7,"箱变标准化:(安全器具：绝缘手套、绝缘靴、操作棒、接地线\\标准化的图文内容：电缆及设备标书牌、二次接线图等)","项",1,null,{"v":0,"d":"0.00"}]
[8,"热缩户内终端头制作，3*70mm2-120mm2","个",1,null,{"v":0,"d":"0.00"},"高压电缆头制作（热缩套管，压接线鼻子、绝缘胶带、孔洞防火泥封堵）"]
[9,"协调费","项",1,null,{"v":0,"d":"0.00"}]
[null,"单项小计",null,null,{"v":0,"d":"0.00"}]
["1、低压部分"]
["序号","项目名称、特征","单位","数量","综合单价/指导价","合价","备注"]
[1,"地上砖砌电缆沟，宽600mm，地上高300mm","m",40,null,{"v":0,"d":"0.00"},"地上电缆沟砌筑（垫层、砌筑、水泥砂浆、回填、盖板、接地网，清运）"]
[2,"水泥井盖，厚度5CM","m",35,null,{"v":0,"d":"0.00"}]
[3,"地上砖砌电缆沟，宽300mm，地上高300mm（电缆沟高度不超过300mm）","m",11,null,{"v":0,"d":"0.00"},"地上电缆沟砌筑（垫层、砌筑、水泥砂浆、回填、盖板、接地网，清运）"]
[4,"水泥井盖，厚度5CM","m",9.625,null,{"v":0,"d":"0.00"}]
[5,"电缆敷设：YJLHV-3*150+2*70mm2","M",120,null,{"v":0,"d":"0.00"},"电缆保护管敷设（配管、锯管、煨弯、管口处理、接管、埋设、接管口）"]
[6,"电缆敷设：YJLHV- 4*150+1*70mm2","M",230,null,{"v":0,"d":"0.00"}]
[7,"热缩终端头制作，150mm2内 五芯","套",34,null,{"v":0,"d":"0.00"}]
[8,"480kW整流柜安装（含现场卸货）","个",2,null,{"v":0,"d":"0.00"}]
[9,"分体式终端安装（含现场卸货）","座",9,null,{"v":0,"d":"0.00"}]
[10,"C25砼浇筑基础，规格：1350*1200mm，高出地坪：200mm","座",2,null,{"v":0,"d":"0.00"},"充电桩基础及箱体安装（人工挖基坑、基地夯实、浇筑混凝土垫层、浇筑混凝土基础、预埋件、回填土、箱体安装、固定预埋件、设备安装含接线）\n"]
[11,"C25砼浇筑基础，规格：500*500mm，高出电缆沟：200mm","座",9,null,{"v":0,"d":"0.00"},"1.充电桩基础及箱体安装（人工挖基坑、基地夯实、浇筑混凝土垫层、浇筑混凝土基础、预埋件、回填土、箱体安装、固定预埋件、设备安装含接线）\n2.含8个直流终端基础、6个交流充电桩基础、1个配电箱基础、4个路灯基础"]
[12,"（充电桩、箱变等）基础表面刷漆，灰色图漆","项",1,null,{"v":0,"d":"0.00"},"基础表面处理和美化"]
[13,"接地扁铁，热镀锌—50X5mm（箱变接地和充电桩接地网连接，）","米",80,null,{"v":0,"d":"0.00"},"防雷接地（设计电阻<4Ω）"]
[14,"接地极（50*5*2500mm镀锌角钢）","根",8,null,{"v":0,"d":"0.00"}]
[15,"磷酸铵盐干粉灭火器（35公斤）手推式","组",1,null,{"v":0,"d":"0.00"},"消防设施"]
[16,"磷酸铵盐干粉灭火器（2*5公斤）手提式","组",4,null,{"v":0,"d":"0.00"}]
[17,"RVV 2*4mm","米",140,null,{"v":0,"d":"0.00"},"含敷设"]
[18,"rvvsp 2*1.5mm","米",140,null,{"v":0,"d":"0.00"},"含敷设"]
[19,"道闸（同进同出）","套","1",null,{"v":0,"d":"0.00"},"1、含对接平台费用\n2、建议采用小鹭管家收费平台\n3、含进出口地感线圈及雷达感应等设备及安装费用\n4、含电源点至道闸供电电缆、人工电缆敷设、电缆保护管及其敷设费用"]
[20,"钢管定位限位器（钢管DN75*3mm），长度2m","套","16",null,{"v":0,"d":"0.00"},"含车挡器安装（预埋板、检查、安装）"]
[21,"停车场本地政府平台对接费用","项","1",null,{"v":0,"d":"0.00"},"停车场本地政府对接预留费用、若无此费用将相应扣除。"]
[22,"引导牌、立招基础安装及电缆敷设","项","1",null,{"v":0,"d":"0.00"},"1、立招及导引牌甲供（立招1个：高4m*宽2m*厚0.2m，导引牌4个：80mm*120mm）\n2、含立招基础制作及安装、供电电缆、供电电缆敷设、地面开挖及恢复\n3、导引牌安装费用"]
[23,"监控照明系统","套","1",null,{"v":0,"d":"0.00"},"1、含400万POE臻全彩高清网络枪型摄像机4组、8路硬盘录像机一组\n2、监控专用硬盘,需保障90天录像\n3、8口POE交换机一只\n4、监控平台\n5、照明设施4根含施工安装（照明品牌建议采用通士达照明）\n6、其他辅材弱电箱\n7、含基础、安装、接地等所有工序     \n8、照明电源采用RVV-2*2.5，网线采用超五类网线，需配置定时器                                    \n9、含3年宽带或3年流量卡，流量卡1年不少于1000G\n10、建议采用海康威视"]
[null,"单项小计",null,null,{"v":0,"d":"0.00"}]
[null,"单项合计",null,null,{"v":0,"d":"0.00"}]
[1,"安全文明施工费","项",1,0.03,{"v":0,"d":"0.00"},"完工后应对场地进行清扫、清洁"]
[2,"税金（施工安装）","项",1,0.09,{"v":0,"d":"0.00"}]
[3,"施工部分合计","项",1,{"v":0,"d":"0.00"}]
["项目总计(一)+（二）",{"$nulls":3},{"v":0,"d":"0.00"},null,"含税"]
["报价单位：                 报价人：                        联系方式："]